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Steel Cleaning – International Practise.
The accepted practise of steel cleaning in preparation of receiving Corrosion Prevention treatment is divided into the categories detailed below.

St2 
This is the internationally accepted standard for cleaning steel pipes as seen on your DVD. It is cleaning by the use of wire brush or similar. This is applicable to all tape systems and is easy to undertake and manage. It will appear on most data sheets.
Sa3 
This is the standard for mechanical cleaning using grit blast or mechanical grinding disc. This is only for liquid coating applications such as the internal of storage tanks. It is known sometimes as white metal cleaning.
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